Files | Functions
OLED Display

Controls the optional 128×64 pixel monochrome OLED display. More...

Collaboration diagram for OLED Display:

## Files
file | display.h

## Functions
int8_t | sb_display_enable ()
| Activate (and setup) the OLED-display. More...
int8_t | sb_display_available ()
| Check if a functional OLED display is present. More...
int8_t | sb_display_disable ()
| Turn the OLED display off. More...
int8_t | sb_display_draw (uint8_t pageNum, uint8_t colNum, uint8_t content)
| Draw a single page segment onto the OLED display. More...
int8_t | sb_display_drawBitmap (uint8_t pageStart, uint8_t colStart, uint8_t pageCount, uint8_t colCount, const uint8_t *contents)
| Draw a (rectangular) bitmap onto the OLED display. More...
int8_t | sb_display_fillScreen (const uint8_t *contents)
| Draw the contents of a `8*128` item 8-bit array (8 pages with 128 columns, each filled with 8 bit) onto the OLED Display. More...
int8_t | sb_display_showString (uint8_t pageNum, uint8_t colStart, const char *str)
| Print a `\0` terminated text string on the OLED display using a 8×8 pixel font. More...
int8_t | sb_display_showStringWide (uint8_t pageNum, uint8_t colStart, const char *str)
| Print a `\0` terminated text string with a (slightly) wider 8×8 pixel font onto the OLED display. More...
int8_t | sb_display_showStringSmall (uint8_t pageNum, uint8_t colStart, const char *str)
| Print a \0 terminated text string on the OLED display using a small 6×4 pixel font. More...

## Detailed Description

Controls the optional 128×64 pixel monochrome OLED display.

The SPiCboard v3 has a TWI (two wire interface, also known as I²C), which can be used to connect an OLED display. Especially the SSD1306 monochrome OLED display fits perfectly onto the board. It has a 0.96 inch diameter with 128 horizontal and 64 vertical pixels.

For the sake of simplicity the horizontal pixels are termed columns. The vertical pixels are divided into 8 so-called pages, therefore a byte can represent the contents of a page segment (with 8 pixels - from the LSB on top to the MSB on bottom of each page segement).

For additional details please have a look into the SSD1306 Datasheet.

In case your run into memory issues (which is quite easy with only 2 KB SRAM) you might want to have a look into the FromFlash function variants.

Warning
  The display is quite sensitive to fluctuation of current. Try to avoid contact of any [semi-]conductive material (including your fingers) with the pins on the Xplained Mini Board – especially connecting PC3 with PC4 – or the connection to your display might stop (it stalls until you restart it, the LED on the Xplained Mini Board can indicate the error).

## Function Documentation

int8_t sb_display_available | ( |  | ) |

Check if a functional OLED display is present.

Tries to connect to the SSD1306 display (I²C device address `0x78`) without enabling it.

Return values

  0 | display is available and seems to work
  <0 | display not available or not functional

int8_t sb_display_disable | ( |  | ) |

Turn the OLED display off.

Return values

  0 | success
  <0 | on I²C error (

See also
  sb_display_enable() return codes)

int8_t sb_display_draw | ( | uint8_t | pageNum,
|  | uint8_t | colNum,
|  | uint8_t | content
| ) |  |

Draw a single page segment onto the OLED display.

Parameters

  pageNum | page number (0-7) for vertical positioning the output
  colNum | column number (0-127) for the horizontal position of the output
  content | contents to be drawn on the page segment (LSB on top and MSB on bottom)

Return values

  0 | success
  <0 | on I²C error (

See also
  sb_display_enable() return codes)

int8_t sb_display_drawBitmap | ( | uint8_t | pageStart,
|  | uint8_t | colStart,
|  | uint8_t | pageCount,
|  | uint8_t | colCount,
|  | const uint8_t * | contents
| ) |  |

Draw a (rectangular) bitmap onto the OLED display.

The result is similar to multiple calls of sb_display_draw() (although the execution of this function is way faster):

for (uint8_t page = 0; page < pageCount; page++){
for (uint8_t col = 0; col < colCount; col++){
sb_display_draw(pageStart + page, colStart + col, contents[page * colCount + col]);
}
}
sb_display_draw
int8_t sb_display_draw(uint8_t pageNum, uint8_t colNum, uint8_t content)
Draw a single page segment onto the OLED display.

Example:

We want to draw a square with a point in its center with some spacing to the to the left top corner of the screen.

The bitmap will be drawn across two pages, each with eight page segments.

Hence we first initialize an array with 2*8 elements (columns 5-12 for page 0 and 1) containing the contents of each page segement (1 for a white pixel and 0 for a black/clear one) and then transfer them to the screen.

#include <stdint.h>
#include <stddef.h>
#include "display.h"
void main(void){
if (sb_display_enable() == 0){ // Enable display (if present)
sb_display_fillScreen(NULL); // Clear display
// Square Bitmap
uint8_t bitmap[] = { 0xF0, 0x10, 0x10, 0x90, 0x90, 0x10, 0x10, 0xF0,
0x0F, 0x08, 0x08, 0x09, 0x09, 0x08, 0x08, 0x0F };
// From PAGE 0 and COLumn 5 draw 2 pages and 8 columns
sb_display_drawBitmap(0, 5, 2, 8, bitmap);
}
while(1); // Stop loop
}
display.h
sb_display_fillScreen
int8_t sb_display_fillScreen(const uint8_t *contents)
Draw the contents of a 8*128 item 8-bit array (8 pages with 128 columns, each filled with 8 bit) onto...
sb_display_enable
int8_t sb_display_enable()
Activate (and setup) the OLED-display.
sb_display_drawBitmap
int8_t sb_display_drawBitmap(uint8_t pageStart, uint8_t colStart, uint8_t pageCount, uint8_t colCount, const uint8_t *contents)
Draw a (rectangular) bitmap onto the OLED display.

Parameters

  pageStart | first page to set the top vertical position
  colStart | first column to set the left horizontal position
  pageCount | number of pages to set the bottom position (including the first page)
  colCount | number of columns to define the right border (including the first column)
  contents | array pointing to the bitmap (must have `pageCount * colCount` elements) - or `NULL` to clear the area

Return values

  0 | success
  <0 | on I²C error (see sb_display_enable() return codes)

int8_t sb_display_enable | ( |  | ) |

Activate (and setup) the OLED-display.

Return values

  0 | success
  -1 | initialization of I²C failed
  -2 | setting I²C device address failed
  -3 | writing to I²C device failed
  -4 | timeout during I²C communication
  -5 | out of bounds (addressing nonexistent page/column)

int8_t sb_display_fillScreen | ( | const uint8_t * | contents | ) |

Draw the contents of a `8*128` item 8-bit array (8 pages with 128 columns, each filled with 8 bit) onto the OLED Display.

The function call is identical to

sb_display_drawBitmap(0, 0, 8, 128, contents);

In case the pointer is `NULL`, the entire screen will be cleared.

Warning
  Make sure that the buffer points to an array with 1024 items - this is C, there is no range check!

Parameters

  contents | pointer to a `8*128` item array - or NULL to clear the screen

Return values

  0 | success
  <0 | on I²C error (

See also
  sb_display_enable() return codes)

int8_t sb_display_showString | ( | uint8_t | pageNum,
|  | uint8_t | colStart,
|  | const char * | str
| ) |  |

Print a `\0` terminated text string on the OLED display using a 8×8 pixel font.

A single character will fit into one page (= eight rows) and eight columns. Therefore it is possible to print 16 characters at maximum.

If the length of the string exceeds the available columns (= columns right of the start column) in the current page, the output will not be continued on the next line!

The font was extract from the Linux kernel and is based on code page 437 (= extended ASCII, every possible character has a graphical string representation).

Consequently, the ASCII control characters (like line break) are displayed with special symbols but don't have any functional impact.

The Fonts Table contains a detailed list of the available characters

Warning
  The font will be stored on the flash which will consume about 2300 bytes.

Parameters

  pageNum | page number (0-7) for vertical positioning the output
  colStart | first column to set the horizontal position of the output
  str | 0-terminated string

Return values

  >=0 | length of printed string (can be less than strlen(str) )
  <0 | on I²C error (

See also
  sb_display_enable() return codes)

int8_t sb_display_showStringSmall | ( | uint8_t | pageNum,
|  | uint8_t | colStart,
|  | const char * | str
| ) |  |

Print a \0 terminated text string on the OLED display using a small 6×4 pixel font.

A single character will fit into one page (eight rows, even though it is just six pixels) and four columns, therefore it is possible to print 32 characters at maximum.

If the length of the string exceeds the available columns (= columns right of the start column) in the current page, the output will not be continued on the next line!

The Fonts Table contains a detailed list of the available characters

Warning
  In contrast to the other `showString` functions the character set is quite limited - it only supports printable ASCII characters (neither control characters nor the extended ASCII set). Hence, the required flash memory consumption is (with about 700 bytes) less than a third of the space requirements of the other fonts.

Parameters

  pageNum | page number (0-7) for vertical positioning the output
  colStart | first column to set the horizontal position of the output
  str | 0-terminated string

Return values

  >=0 | length of printed string (can be less than strlen(str) )
  <0 | on I²C error (

See also
  sb_display_enable() return codes)

int8_t sb_display_showStringWide | ( | uint8_t | pageNum,
|  | uint8_t | colStart,
|  | const char * | str
| ) |  |

Print a `\0` terminated text string with a (slightly) wider 8×8 pixel font onto the OLED display.

The character set is almost identical to the sb_display_showString() function and the space requirement is the same (up to 16 characters per line)

The Fonts Table contains a detailed list of the available characters.

Warning
  This font will consume about 2300 bytes, too.

Parameters

  pageNum | page number (0-7) for vertical positioning the output
  colStart | first column to set the horizontal position of the output
  str | 0-terminated string

Return values

  >=0 | length of printed string (can be less than strlen(str) )
  <0 | on I²C error (see sb_display_enable() return codes)