Files | Enumerations | Functions
ADC (Analog to Digital Converter)

Interface to the AD-converter of the ATmega32, which allows to query the potentiometer and the photosensor of the board. More...

## Files
file | adc.h

## Enumerations
enum | ADCDEV { POTI , PHOTO }
| Device ids of available periphery connected to ADC channels. More...

## Functions
int16_t | sb_adc_read (ADCDEV dev)
| Perform a 10-bit A/D conversion for a specific channel/device. More...

## Detailed Description

Interface to the AD-converter of the ATmega32, which allows to query the potentiometer and the photosensor of the board.

## Enumeration Type Documentation

enum ADCDEV

Device ids of available periphery connected to ADC channels.

Enumerator
POTI | the potentiometer (rotation towards LEDs yields higher numbers)
PHOTO | the photosensor (brighter ambience yields higher numbers)

## Function Documentation

int16_t sb_adc_read | ( | ADCDEV | dev | ) |

Perform a 10-bit A/D conversion for a specific channel/device.

Parameters

  dev | id of a device connected to the ADC

Return values

  >=0 | 10-bit result of the conversion
  -1 | invalid device id